|  |  |  |
| --- | --- | --- |
| **Subject:** | AllCutter Driver | |
| **Versions:** | V2.46-02 | **Release date:**  2025/08/26 |

# Problem Fixed

1. Fix the issue where the cutting direction cannot be set to clockwise for circular objects with diameter smaller than 10 mm.
2. Fix the issue that “Use Extended Blade Holder” item was not shown in RXII driver.
3. Fix the issue on RXII that “Die Cut” function cannot work if AAS mark plugin is running and “section cut” was enabled.

# New Functions Added

N/A

# Problem or Known Limitation

N/A

# Appendices

N/A